Protel Design System Design Rule Check
PCB File : M:\Otworowanie\Sonda_RPi.PcbDoc
Date     : 2018-06-13
Time     : 13:58:57

Processing Rule : Clearance Constraint (Gap=0.152mm) (All),(All)
   Violation between Clearance Constraint: (0.152mm < 0.152mm) Between Region (0 hole(s)) Bottom Layer And Track (106.932mm,47.844mm)(110.737mm,47.844mm) on Bottom Layer 
   Violation between Clearance Constraint: (0.152mm < 0.152mm) Between Region (0 hole(s)) Bottom Layer And Track (110.737mm,47.844mm)(110.91mm,47.671mm) on Bottom Layer 
   Violation between Clearance Constraint: (0.15mm < 0.152mm) Between Region (0 hole(s)) Bottom Layer And Track (89.607mm,89.683mm)(89.607mm,90.202mm) on Bottom Layer 
   Violation between Clearance Constraint: (0.15mm < 0.152mm) Between Region (0 hole(s)) Bottom Layer And Track (89.607mm,89.683mm)(89.807mm,89.483mm) on Bottom Layer 
Rule Violations :4

Processing Rule : Short-Circuit Constraint (Allowed=No) (All),(All)
   Violation between Short-Circuit Constraint: Between Via (126.375mm,62.325mm) from Top Layer to Bottom Layer And Pad MOTOR1-M(126.95mm,62.325mm) on Top Layer Location : [X = 126.375mm][Y = 62.325mm]
   Violation between Short-Circuit Constraint: Between Via (127.525mm,62.325mm) from Top Layer to Bottom Layer And Pad MOTOR1-M(126.95mm,62.325mm) on Top Layer Location : [X = 127.525mm][Y = 62.325mm]
   Violation between Short-Circuit Constraint: Between Area Fill (126.05mm,52.35mm) (127.85mm,74.1mm) on Top Layer And Pad MOTOR1-M(126.95mm,62.325mm) on Top Layer Location : [X = 126.95mm][Y = 62.325mm]
   Violation between Short-Circuit Constraint: Between Via (127.525mm,52.95mm) from Top Layer to Bottom Layer And Pad MOTOR1-M(126.95mm,52.95mm) on Top Layer Location : [X = 127.525mm][Y = 52.95mm]
   Violation between Short-Circuit Constraint: Between Via (126.375mm,52.95mm) from Top Layer to Bottom Layer And Pad MOTOR1-M(126.95mm,52.95mm) on Top Layer Location : [X = 126.375mm][Y = 52.95mm]
   Violation between Short-Circuit Constraint: Between Area Fill (126.05mm,52.35mm) (127.85mm,74.1mm) on Top Layer And Pad MOTOR1-M(126.95mm,52.95mm) on Top Layer Location : [X = 126.95mm][Y = 52.95mm]
   Violation between Short-Circuit Constraint: Between Via (126.375mm,73.5mm) from Top Layer to Bottom Layer And Pad MOTOR2-M(126.95mm,73.5mm) on Top Layer Location : [X = 126.375mm][Y = 73.5mm]
   Violation between Short-Circuit Constraint: Between Via (127.525mm,73.5mm) from Top Layer to Bottom Layer And Pad MOTOR2-M(126.95mm,73.5mm) on Top Layer Location : [X = 127.525mm][Y = 73.5mm]
   Violation between Short-Circuit Constraint: Between Area Fill (126.05mm,52.35mm) (127.85mm,74.1mm) on Top Layer And Pad MOTOR2-M(126.95mm,73.5mm) on Top Layer Location : [X = 126.95mm][Y = 73.5mm]
   Violation between Short-Circuit Constraint: Between Via (127.525mm,64.15mm) from Top Layer to Bottom Layer And Pad MOTOR2-M(126.95mm,64.125mm) on Top Layer Location : [X = 127.525mm][Y = 64.15mm]
   Violation between Short-Circuit Constraint: Between Via (126.375mm,64.15mm) from Top Layer to Bottom Layer And Pad MOTOR2-M(126.95mm,64.125mm) on Top Layer Location : [X = 126.375mm][Y = 64.15mm]
   Violation between Short-Circuit Constraint: Between Area Fill (126.05mm,52.35mm) (127.85mm,74.1mm) on Top Layer And Pad MOTOR2-M(126.95mm,64.125mm) on Top Layer Location : [X = 126.95mm][Y = 64.125mm]
Rule Violations :12

Processing Rule : Un-Routed Net Constraint ( (All) )
   Violation between Un-Routed Net Constraint: Net 3.3V Between Pad RPi1-1(68.49mm,91.685mm) on Multi-Layer And Via (83.375mm,90.175mm) from Top Layer to Bottom Layer 
Rule Violations :1

Processing Rule : Power Plane Connect Rule(Relief Connect )(Expansion=0.608mm) (Conductor Width=0.4mm) (Air Gap=0.254mm) (Entries=4) (All)
Rule Violations :0


Violations Detected : 17
Time Elapsed        : 00:00:01